Leica Runner 24 Automatic Optical Level - Level Only

The Leica Runner 24 with its x24 magnification is a robust and mid-priced automatic builder's levels. Designed to work hard on the job site. They are quick to set up, simple to use and very reliable. The automatic compensator and the fast optics speed up measurements onsite and increase accuracy.

**Featured with**
 Robust and accurate
 Air-damped compensator with control button
 Water resistant (IP55)
 Double-sided endless fine drive for easy   targeting
 Penta Prism for easy viewing of circular   level
 Horizontal circle with 360° division



**When choosing When choosing a level the quality of the optics if often overlooked.**

All Leica levels feature best in class Swiss lenses & optics which give a far superior quality and sharpness of image over that of generic brands.

The Leica Runner  range include many features not seen on other levels such as super fine double sided endless targeting for fine adjustment of the level and magnetic air-dampened compensator for super stable images.

RUNNER 20 / 24 Kits are robust and value-priced automatic builder's / dumpy level Packages containing a Runner 20 / Runner 24 Level, Tripod & Levelling Staff. Designed to work hard on the job site. It is quick to set up, simple to use and very reliable. The automatic compensator and the fast optics speed up measurements onsite and increase accuracy. RUNNER -- the ideal partner for your daily levelling tasks.

These levels are unshakeable. With a level from Leica you can just keep on working.

RUNNER is the ideal construction level for site foremen ,engineers, architects, landscape gardeners, carpenters, construction companies and many more.

Build to Last - Levels for Construction and Engineering Surveys

RUNNER means superior performance at a great price

  Air-damped compensator with control button
  Water resistant (IP55)
  Double-sided endless fine drive for easy targeting
  Pentaprism for easy viewing of circular level
  Horizontal circle with 360° division
  Value-priced

|  |  |  |
| --- | --- | --- |
| **Technical Data** | [RUNNER 20 KIT](http://www.merlinlazer.com/Leica-Runner-20-Automatic-Optical-Level-KIT-Includes-Runner-Tripod-Levelling-Staff) | [RUNNER 24 KIT](http://www.merlinlazer.com/Leica-Runner-24-Automatic-Optical-Level-KIT-Includes-Runner-Tripod-Levelling-Staff) |
| **Accuracy per km double-run leveling** | 2.5 mm | 2.0 mm |
| **Magnification** | 20x | 24x |
| **Shortest focusing distance** | 0.8 m | 0.8 m |
| **Compensator** |   |   |
|   Working range | ±15' | ±15' |
|   Setting accuracy | 0.5" | 0.5" |
| **Operating temperature** | -20°C to +50°C | -20°C to +50°C |
| **Weight (net)** | 2 kg | 2 kg |

**Kit Contains:**
1No: Leica Runner 20 or Leica Runner 24 Automatic Optical Builders Level
1No: Tripod
1No: 5m Levelling Staff